MPLS-SETUP-PIB PIB-DEFINITIONS ::= BEGIN 
 
IMPORTS 
   MODULE-IDENTITY, OBJECT-TYPE,  
   TEXTUAL-CONVENTION, MODULE-COMPLIANCE,  
   OBJECT-IDENTITY, OBJECT-GROUP 
      FROM COPS-PR-SPPI 
   TruthValue 
         FROM SNMPv2-TC 
   InstanceId, ReferenceId, TagId, TagReference 
         FROM COPS-PR-SPPI-TC 
   SnmpAdminString 
         FROM SNMP-FRAMEWORK-MIB 
   InetAddressIPv4, InetAddressIPv6 
         FROM INET-ADDRESS-MIB 
 
mplsSetupPib MODULE-IDENTITY 
   SUBJECT-CATEGORIES SUBJECT-CATEGORY { tbd “ MPLS Setup Client 
Type } 
   LAST-UPDATED "200107131000Z" 
   ORGANIZATION " WG" 
   CONTACT-INFO " 
                Harsha Hegde 
                Intel Corporation 
                MS JF3-206 
                2111 NE 25th Ave. 
                Hillsboro, OR 97124 
                Phone: +1 503 264 1439 
                Fax: +1 503 264 3483 
                E-Mail: shriharsha.hegde@intel.com 
 
                Ravi Sahita   
                Intel Corporation 
                JF3-206            
                2111 NE 25th Ave   
                Hillsboro, Oregon 97124   
                Phone: +1 503 264 1439 
                Fax: +1 503 264 3483 
                Email: ravi.sahita@intel.com 
                " 
   DESCRIPTION 
         "This PIB module contains a set of provisioning classes 

         that are used to setup MPLS LSPs on MPLS Routers." 
   ::= { tbd } 
 
 
-- 
-- Forward Equivalence Class (FEC) Classes 
-- 
 
mplsFecClasses  OBJECT IDENTIFIER ::= { mplsSetupPib 1 } 
 
-- 
-- IPv4 Host Address FEC Table 
-- 
 
mplsFecIPv4HostAddrTable OBJECT-TYPE 
    SYNTAX         SEQUENCE OF MplsFecIPv4HostAddrEntry 
    PIB-ACCESS     install 
    STATUS         current 
    DESCRIPTION 
        "This table consists of MPLS IPv4 FEC Entrees." 
 
    ::= { mplsFecClasses  1 } 
 
mplsFecIPv4HostAddrEntry OBJECT-TYPE 
    SYNTAX         MplsFecIPv4HostAddrEntry 
    STATUS         current 
    DESCRIPTION 
        "An instance of this class describes MPLS IPv4 Host Address 
        FEC. " 
 
    PIB-INDEX { mplsFecIPv4HostAddrPrid } 
 
    ::= { mplsFecIPv4HostAddrTable 1 } 
 
MplsFecIPv4HostAddrEntry ::= SEQUENCE { 
        mplsFecIPv4HostAddrPrid        InstanceId, 
        mplsFecIPv4HostAddrIpAddr      InetAddressIPv4 } 
 
mplsFecIPv4HostAddrPrid OBJECT-TYPE 
    SYNTAX         InstanceId 
    STATUS         current 
    DESCRIPTION 
        "An integer index that uniquely identifies an instance of 
        the mplsFecIPv4HostAddrEntry class." 
 
    ::= { mplsFecIPv4HostAddrEntry 1 } 
 
mplsFecIPv4HostAddrIpAddr OBJECT-TYPE 
    SYNTAX         InetAddressIPv4 
    STATUS         current 
    DESCRIPTION 
        "IPv4 Host Address in a FEC." 
 

    ::= { mplsFecIPv4HostAddrEntry 2 } 
 
 
-- 
-- IPv6 Host Address FEC Table 
-- 
 
mplsFecIPv6HostAddrTable OBJECT-TYPE 
    SYNTAX         SEQUENCE OF MplsFecIPv6HostAddrEntry 
    PIB-ACCESS     install 
    STATUS         current 
    DESCRIPTION 
        "This table consists of MPLS IPv6 FEC entrees." 
 
    ::= { mplsFecClasses  2 } 
 
mplsFecIPv6HostAddrEntry OBJECT-TYPE 
    SYNTAX         MplsFecIPv6HostAddrEntry 
    STATUS         current 
    DESCRIPTION 
        "An instance of this class describes an IPv6 Host Address 
        FEC. " 
 
    PIB-INDEX { mplsFecIPv6HostAddrPrid } 
 
    ::= { mplsFecIPv6HostAddrTable 1 } 
 
MplsFecIPv6HostAddrEntry ::= SEQUENCE { 
        mplsFecIPv6HostAddrPrid        InstanceId, 
        mplsFecIPv6HostAddrIpAddr      InetAddressIPv6 } 
 
mplsFecIPv6HostAddrPrid OBJECT-TYPE 
    SYNTAX         InstanceId 
    STATUS         current 
    DESCRIPTION 
        "An integer index that uniquely identifies an instance of 
        the mplsFecIPv6HostAddrEntry class." 
 
    ::= { mplsFecIPv6HostAddrEntry 1 } 
 
mplsFecIPv6HostAddrIpAddr OBJECT-TYPE 
    SYNTAX         InetAddressIPv6 
    STATUS         current 
    DESCRIPTION 
        "IPv6 Host Address in a FEC." 
 
    ::= { mplsFecIPv6HostAddrEntry 2 } 
 
 
-- 
-- IPv4 Prefix FEC Table 
-- 
 

mplsFecIPv4PrefixTable OBJECT-TYPE 
    SYNTAX         SEQUENCE OF MplsFecIPv4PrefixEntry 
    PIB-ACCESS     install 
    STATUS         current 
    DESCRIPTION 
        "This table consists of MPLS IPv4 Prefix FEC entrees." 
 
    ::= { mplsFecClasses  3 } 
 
mplsFecIPv4PrefixEntry OBJECT-TYPE 
    SYNTAX         MplsFecIPv4PrefixEntry 
    STATUS         current 
    DESCRIPTION 
        "An instance of this class describes a IPv4 Prefix FEC." 
 
    PIB-INDEX { mplsFecIPv4PrefixPrid } 
 
    ::= { mplsFecIPv4PrefixTable 1 } 
 
MplsFecIPv4PrefixEntry ::= SEQUENCE { 
        mplsFecIPv4PrefixPrid        InstanceId, 
        mplsFecIPv4PrefixLength      Unsigned32, 
        mplsFecIPv4PrefixIpPrefix    InetAddressIPv4 } 
 
mplsFecIPv4PrefixPrid OBJECT-TYPE 
    SYNTAX         InstanceId 
    STATUS         current 
    DESCRIPTION 
        "An integer index that uniquely identifies an instance of 
        the mplsFecIPv4PrefixEntry class." 
 
    ::= { mplsFecIPv4PrefixEntry 1 } 
 
mplsFecIPv4PrefixLength OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Length of IPv4 Prefix in a FEC." 
 
    ::= { mplsFecIPv4PrefixEntry 2 } 
 
mplsFecIPv4PrefixIpPrefix OBJECT-TYPE 
    SYNTAX         InetAddressIPv4 
    STATUS         current 
    DESCRIPTION 
        "IPv4 Prefix in a FEC." 
 
    ::= { mplsFecIPv4PrefixEntry 3 } 
 
 
-- 
-- IPv6 Prefix FEC Table 
-- 

 
mplsFecIPv6PrefixTable OBJECT-TYPE 
    SYNTAX         SEQUENCE OF MplsFecIPv6PrefixEntry 
    PIB-ACCESS     install 
    STATUS         current 
    DESCRIPTION 
        "This table consists of MPLS IPv6 Prefix FEC entrees." 
 
    ::= { mplsFecClasses  4 } 
 
mplsFecIPv6PrefixEntry OBJECT-TYPE 
    SYNTAX         MplsFecIPv6PrefixEntry 
    STATUS         current 
    DESCRIPTION 
        "An instance of this class describes a IPv6 Prefix FEC." 
 
    PIB-INDEX { mplsFecIPv6PrefixPrid } 
 
    ::= { mplsFecIPv6PrefixTable 1 } 
 
MplsFecIPv6PrefixEntry ::= SEQUENCE { 
        mplsFecIPv6PrefixPrid        InstanceId, 
        mplsFecIPv6PrefixLength      Unsigned32, 
        mplsFecIPv6PrefixIpPrefix    InetAddressIPv6 } 
 
mplsFecIPv6PrefixPrid OBJECT-TYPE 
    SYNTAX         InstanceId 
    STATUS         current 
    DESCRIPTION 
        "An integer index that uniquely identifies an instance of 
        the mplsFecIPv6PrefixEntry class." 
 
    ::= { mplsFecIPv6PrefixEntry 1 } 
 
mplsFecIPv6PrefixLength OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Length of IPv6 Prefix in a FEC." 
 
    ::= { mplsFecIPv6PrefixEntry 2 } 
 
mplsFecIPv6PrefixIpPrefix OBJECT-TYPE 
    SYNTAX         InetAddressIPv6 
    STATUS         current 
    DESCRIPTION 
        "IPv6 Prefix in a FEC." 
 
    ::= { mplsFecIPv6PrefixEntry 3 } 
 
 
-- 
-- Autonomous System Number FEC Table 

-- 
 
mplsFecASTable OBJECT-TYPE 
    SYNTAX         SEQUENCE OF MplsFecASEntry 
    PIB-ACCESS     install 
    STATUS         current 
    DESCRIPTION 
        "This table consists of MPLS Autonomous System Number FEC 
        entrees." 
 
    ::= { mplsFecClasses  5 } 
 
mplsFecASEntry OBJECT-TYPE 
    SYNTAX         MplsFecASEntry 
    STATUS         current 
    DESCRIPTION 
        "An instance of this class describes an Autonomous System 
        Number FEC. " 
 
    PIB-INDEX { mplsFecASPrid } 
 
    ::= { mplsFecASTable 1 } 
 
MplsFecASEntry ::= SEQUENCE { 
        mplsFecASPrid        InstanceId, 
        mplsFecASNumber      Unsigned32 } 
 
mplsFecASPrid OBJECT-TYPE 
    SYNTAX         InstanceId 
    STATUS         current 
    DESCRIPTION 
        "An integer index that uniquely identifies an instance of 
        the mplsFecASEntry class." 
 
    ::= { mplsFecASEntry 1 } 
 
mplsFecASNumber OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Autonomous System Number in a FEC." 
 
    ::= { mplsFecASEntry 2 } 
 
 
-- 
-- Label Request Classes 
-- 
 
mplsLabReqClasses  OBJECT IDENTIFIER ::= { mplsSetupPib 2 } 
 
-- 
-- Generic Label Request Table 

-- 
 
mplsLabReqGenericTable OBJECT-TYPE 
    SYNTAX         SEQUENCE OF MplsLabReqGenericEntry 
    PIB-ACCESS     install 
    STATUS         current 
    DESCRIPTION 
        "This table consists of MPLS Generic Label Request Object 
        entrees." 
 
    ::= { mplsLRClasses  1 } 
 
mplsLabReqGenericEntry OBJECT-TYPE 
    SYNTAX         MplsLabReqGenericEntry 
    STATUS         current 
    DESCRIPTION 
        "An instance of this class describes MPLS Generic Label 
        Request Object. " 
 
    PIB-INDEX { mplsLabReqGenericPrid } 
 
    ::= { mplsLabReqGenericTable 1 } 
 
MplsLabReqGenericEntry ::= SEQUENCE { 
        mplsLabReqGenericPrid        InstanceId, 
        mplsLabReqGenericL3Pid       Unsigned32 } 
 
mplsLabReqGenericPrid OBJECT-TYPE 
    SYNTAX         InstanceId 
    STATUS         current 
    DESCRIPTION 
        "An integer index that uniquely identifies an instance of 
        the mplsLabReqGenericEntry class." 
 
    ::= { mplsLabReqGenericEntry 1 } 
 
mplsLabReqGenericL3Pid OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Layer 3 Protocol Id in MPLS Generic Label Request 
        Object." 
 
    ::= { mplsLabReqGenericEntry 2 } 
 
 
-- 
-- ATM Label Request Table 
-- 
 
mplsLabReqATMTable OBJECT-TYPE 
    SYNTAX         SEQUENCE OF MplsLabReqATMEntry 
    PIB-ACCESS     install 

    STATUS         current 
    DESCRIPTION 
        "This table consists of MPLS ATM Label Request Object 
        entrees." 
 
    ::= { mplsLabReqClasses  1 } 
 
mplsLabReqATMEntry OBJECT-TYPE 
    SYNTAX         MplsLabReqATMEntry 
    STATUS         current 
    DESCRIPTION 
        "An instance of this class describes MPLS ATM Label 
        Request Object. " 
 
    PIB-INDEX { mplsLabReqATMPrid } 
 
    ::= { mplsLabReqATMTable 1 } 
 
MplsLabReqATMEntry ::= SEQUENCE { 
        mplsLabReqATMPrid        InstanceId, 
        mplsLabReqATML3Pid       Unsigned32, 
        mplsLabReqATMMbit        Unsigned32, 
        mplsLabReqATMMinVpi      Unsigned32, 
        mplsLabReqATMMaxVpi      Unsigned32, 
        mplsLabReqATMMinVci      Unsigned32, 
        mplsLabReqATMMaxVci      Unsigned32 } 
 
mplsLabReqATMPrid OBJECT-TYPE 
    SYNTAX         InstanceId 
    STATUS         current 
    DESCRIPTION 
        "An integer index that uniquely identifies an instance of 
        the mplsLabReqATMEntry class." 
 
    ::= { mplsLabReqATMEntry 1 } 
 
mplsLabReqATML3Pid OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Layer 3 Protocol Id in MPLS ATM Label Request 
        Object." 
 
    ::= { mplsLabReqATMEntry 2 } 
 
mplsLabReqATMMbit OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Merging Capable Bit in MPLS ATM Label Request Object." 
 
    ::= { mplsLabReqATMEntry 3 } 
 

mplsLabReqATMMinVpi OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Minimum value for VPI in MPLS ATM Label Request Object." 
 
    ::= { mplsLabReqATMEntry 4 } 
 
mplsLabReqATMMaxVpi OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Maximum value for VPI in MPLS ATM Label Request Object." 
 
    ::= { mplsLabReqATMEntry 5 } 
 
mplsLabReqATMMinVci OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Minimum value for VCI in MPLS ATM Label Request Object." 
 
    ::= { mplsLabReqATMEntry 6 } 
 
mplsLabReqATMMaxVci OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Maximum value for VCI in MPLS ATM Label Request Object." 
 
    ::= { mplsLabReqATMEntry 7 } 
 
 
-- 
-- Frame Relay Label Request Table 
-- 
 
mplsLabReqFRTable OBJECT-TYPE 
    SYNTAX         SEQUENCE OF MplsLabReqFREntry 
    PIB-ACCESS     install 
    STATUS         current 
    DESCRIPTION 
        "This table consists of MPLS Frame Relay Label Request 
        Object entrees." 
 
    ::= { mplsLabReqClasses  1 } 
 
mplsLabReqFREntry OBJECT-TYPE 
    SYNTAX         MplsLabReqFREntry 
    STATUS         current 
    DESCRIPTION 
        "An instance of this class describes MPLS Frame Relay 
        Label Request Object. " 

 
    PIB-INDEX { mplsLabReqFRPrid } 
 
    ::= { mplsLabReqFRTable 1 } 
 
MplsLabReqFREntry ::= SEQUENCE { 
        mplsLabReqFRPrid        InstanceId, 
        mplsLabReqFRL3Pid       Unsigned32, 
        mplsLabReqFRDlciLen     Unsigned32, 
        mplsLabReqFRMinDlci     Unsigned32, 
        mplsLabReqFRMaxDlci     Unsigned32} 
 
mplsLabReqFRPrid OBJECT-TYPE 
    SYNTAX         InstanceId 
    STATUS         current 
    DESCRIPTION 
        "An integer index that uniquely identifies an instance of 
        the mplsLabReqFREntry class." 
 
    ::= { mplsLabReqFREntry 1 } 
 
mplsLabReqFRL3Pid OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Layer 3 Protocol Id in MPLS Frame Relay Label Request 
        Object." 
 
    ::= { mplsLabReqFREntry 2 } 
 
mplsLabReqFRDlciLen OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Length of DLCI in MPLS Frame Relay Label Request Object." 
 
    ::= { mplsLabReqFREntry 3 } 
 
mplsLabReqFRMinDlci OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Minimum value DLCI in MPLS Frame Relay Label Request 
        Object." 
 
    ::= { mplsLabReqFREntry 4 } 
 
mplsLabReqFRMaxDlci OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Maximum value DLCI in MPLS Frame Relay Label Request 
        Object." 

 
    ::= { mplsLabReqFREntry 5 } 
 
 
-- 
-- Flow (Traffic) Specification Classes 
-- 
 
mplsFlowSpecClasses  OBJECT IDENTIFIER ::= { mplsSetupPib 3 } 
 
-- 
-- CRLDP Flow Spec Table 
-- 
 
mplsFlowSpecCRLDPTable OBJECT-TYPE 
    SYNTAX         SEQUENCE OF MplsFlowSpecCRLDPEntry 
    PIB-ACCESS     install 
    STATUS         current 
    DESCRIPTION 
        "This table consists of CR-LDP Traffic (Flow) Specification  
        entrees." 
 
    ::= { mplsFlowSpecClasses  1 } 
 
mplsFlowSpecCRLDPEntry OBJECT-TYPE 
    SYNTAX         MplsFlowSpecCRLDPEntry 
    STATUS         current 
    DESCRIPTION 
        "An instance of this class describes a CR-LDP Flow 
        Specification. " 
 
    PIB-INDEX { mplsFlowSpecCRLDPPrid } 
 
    ::= { mplsFlowSpecCRLDPTable 1 } 
 
MplsFlowSpecCRLDPEntry ::= SEQUENCE { 
        mplsFlowSpecCRLDPPrid    InstanceId, 
        mplsFlowSpecCRLDPPDR     Unsigned32, 
        mplsFlowSpecCRLDPPBS     Unsigned32, 
        mplsFlowSpecCRLDPCDR     Unsigned32, 
        mplsFlowSpecCRLDPCBS     Unsigned32, 
        mplsFlowSpecCRLDPEBS     Unsigned32, 
        mplsFlowSpecCRLDPWeight  Unsigned32 } 
 
mplsFlowSpecCRLDPPrid OBJECT-TYPE 
    SYNTAX         InstanceId 
    STATUS         current 
    DESCRIPTION 
        "An integer index that uniquely identifies an instance of 
        the mplsFlowSpecCRLDPEntry class." 
 
    ::= { mplsFlowSpecCRLDPEntry 1 } 
 

mplsFlowSpecCRLDPPDR OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Peak Data Rate in CR-LDP Flow Specification." 
 
    ::= { mplsFlowSpecCRLDPEntry 2 } 
 
mplsFlowSpecCRLDPPBS OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Peak Burst Size in CR-LDP Flow Specification." 
 
    ::= { mplsFlowSpecCRLDPEntry 3 } 
 
mplsFlowSpecCRLDPCDR OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Committed Data Rate in CR-LDP Flow Specification." 
 
    ::= { mplsFlowSpecCRLDPEntry 4 } 
 
mplsFlowSpecCRLDPCBS OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Committed Burst Size in CR-LDP Flow Specification." 
 
 
    ::= { mplsFlowSpecCRLDPEntry 5 } 
 
mplsFlowSpecCRLDPEBS OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Excess Burst Size in CR-LDP Flow Specification." 
 
    ::= { mplsFlowSpecCRLDPEntry 6 } 
 
mplsFlowSpecCRLDPWeight OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Weight parameter in CR-LDP Flow Specification." 
 
    ::= { mplsFlowSpecCRLDPEntry 7 } 
 
 
-- 
-- RSVP Controlled Load Service Flow Spec Table 
-- 

 
mplsFlowSpecCLSTable OBJECT-TYPE 
    SYNTAX         SEQUENCE OF MplsFlowSpecCLSEntry 
    PIB-ACCESS     install 
    STATUS         current 
    DESCRIPTION 
        "This table consists of RSVP-TE Integrated Services 
        (IntServ) Controlled Load Service Flow Specification 
        entrees." 
 
    ::= { mplsFlowSpecClasses  2 } 
 
mplsFlowSpecCLSEntry OBJECT-TYPE 
    SYNTAX         MplsFlowSpecCLSEntry 
    STATUS         current 
    DESCRIPTION 
        "An instance of this class describes RSVP-TE IntServ 
        Controlled Load Service Flow Specification. " 
 
    PIB-INDEX { mplsFlowSpecCLSPrid } 
 
    ::= { mplsFlowSpecCLSTable 1 } 
 
MplsFlowSpecCLSEntry ::= SEQUENCE { 
        mplsFlowSpecCLSPrid        InstanceId, 
        mplsFlowSpecCLSTokenRate   Unsigned32, 
        mplsFlowSpecCLSBucketSize  Unsigned32, 
        mplsFlowSpecCLSPeakRate    Unsigned32, 
        mplsFlowSpecCLSMinPoliced  Unsigned32, 
        mplsFlowSpecCLSMaxPktSize  Unsigned32 } 
 
mplsFlowSpecCLSPrid OBJECT-TYPE 
    SYNTAX         InstanceId 
    STATUS         current 
    DESCRIPTION 
        "An integer index that uniquely identifies an instance of 
        the mplsFlowSpecCLSEntry class." 
 
    ::= { mplsFlowSpecCLSEntry 1 } 
 
mplsFlowSpecCLSTokenRate OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Token Rate in RSVP-TE IntServ Controlled Load Service  
        Flow Specification." 
 
    ::= { mplsFlowSpecCLSEntry 2 } 
 
mplsFlowSpecCLSBucketSize OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 

        "Token Bucket Size in RSVP-TE IntServ Controlled Load 
        Service Flow Specification." 
 
    ::= { mplsFlowSpecCLSEntry 3 } 
 
mplsFlowSpecCLSPeakRate OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Peak Rate in RSVP-TE IntServ Controlled Load Service  
        Flow Specification." 
 
    ::= { mplsFlowSpecCLSEntry 4 } 
 
mplsFlowSpecCLSMinPoliced OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Minimum Policed Packet Size in RSVP-TE IntServ Controlled 
        Load Service Flow Specification." 
 
    ::= { mplsFlowSpecCLSEntry 5 } 
 
mplsFlowSpecCLSMaxPktSize OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Maximum Packet Size in RSVP-TE IntServ Controlled Load 
        Service Flow Specification." 
 
    ::= { mplsFlowSpecCLSEntry 6 } 
 
 
 
-- 
-- RSVP Guaranteed Service Flow Spec Table 
-- 
 
mplsFlowSpecGSTable OBJECT-TYPE 
    SYNTAX         SEQUENCE OF MplsFlowSpecGSEntry 
    PIB-ACCESS     install 
    STATUS         current 
    DESCRIPTION 
        "This table consists of RSVP-TE Integrated Services 
        (IntServ) Guaranteed Service Flow Specification entrees." 
 
    ::= { mplsFlowSpecClasses  3 } 
 
mplsFlowSpecGSEntry OBJECT-TYPE 
    SYNTAX         MplsFlowSpecGSEntry 
    STATUS         current 
    DESCRIPTION 
        "An instance of this class describes RSVP-TE IntServ 

        Guaranteed Service Flow Specification. " 
 
    PIB-INDEX { mplsFlowSpecGSPrid } 
 
    ::= { mplsFlowSpecGSTable 1 } 
 
MplsFlowSpecGSEntry ::= SEQUENCE { 
        mplsFlowSpecGSPrid        InstanceId, 
        mplsFlowSpecGSTokenRate   Unsigned32, 
        mplsFlowSpecGSBucketSize  Unsigned32, 
        mplsFlowSpecGSPeakRate    Unsigned32, 
        mplsFlowSpecGSMinPoliced  Unsigned32, 
        mplsFlowSpecGSMaxPktSize  Unsigned32, 
        mplsFlowSpecGSRspecRate   Unsigned32, 
        mplsFlowSpecGSSlackTerm   Unsigned32 } 
 
mplsFlowSpecGSPrid OBJECT-TYPE 
    SYNTAX         InstanceId 
    STATUS         current 
    DESCRIPTION 
        "An integer index that uniquely identifies an instance of 
        the mplsFlowSpecGSEntry class." 
 
    ::= { mplsFlowSpecGSEntry 1 } 
 
mplsFlowSpecGSTokenRate OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Token Rate in RSVP-TE IntServ Guaranteed Service  
        Flow Specification." 
 
    ::= { mplsFlowSpecGSEntry 2 } 
 
mplsFlowSpecGSBucketSize OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Token Bucket Size in RSVP-TE IntServ Guaranteed 
        Service Flow Specification." 
 
    ::= { mplsFlowSpecGSEntry 3 } 
 
mplsFlowSpecGSPeakRate OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Peak Rate in RSVP-TE IntServ Guaranteed Service  
        Flow Specification." 
 
    ::= { mplsFlowSpecGSEntry 4 } 
 
mplsFlowSpecGSMinPoliced OBJECT-TYPE 

    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Minimum Policed Packet Size in RSVP-TE IntServ Guaranteed 
        Service Flow Specification." 
 
    ::= { mplsFlowSpecGSEntry 5 } 
 
mplsFlowSpecGSMaxPktSize OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Maximum Packet Size in RSVP-TE IntServ Guaranteed 
        Service Flow Specification." 
 
    ::= { mplsFlowSpecGSEntry 6 } 
 
mplsFlowSpecGSRspecRate OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Required Rate in RSVP-TE IntServ Guaranteed Service  
        Flow Specification." 
 
    ::= { mplsFlowSpecGSEntry 7 } 
 
mplsFlowSpecGSSlackTerm OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Slack Term (Delay) in RSVP-TE IntServ Guaranteed Service  
        Flow Specification." 
 
    ::= { mplsFlowSpecGSEntry 8 } 
 
 
-- 
-- Explicit Route Object (ERO) Classes 
-- 
 
mplsEroClasses  OBJECT IDENTIFIER ::= { mplsSetupPib 4 } 
 
-- 
-- IPv4 Address Prefix Subobject Table 
-- 
 
mplsEroIPv4PrefixTable OBJECT-TYPE 
    SYNTAX         SEQUENCE OF MplsEroIPv4PrefixEntry 
    PIB-ACCESS     install 
    STATUS         current 
    DESCRIPTION 
        "This table consists of MPLS IPv4 Prefix ERO Subobject 
        Entrees." 

 
    ::= { mplsEroClasses  1 } 
 
mplsEroIPv4PrefixEntry OBJECT-TYPE 
    SYNTAX         MplsEroIPv4PrefixEntry 
    STATUS         current 
    DESCRIPTION 
        "An instance of this class describes IPv4 Prefix ERO 
        Subobject. "                                        
 
    PIB-INDEX { mplsEroIPv4PrefixPrid } 
 
    ::= { mplsEroIPv4PrefixTable 1 } 
 
MplsEroIPv4PrefixEntry ::= SEQUENCE { 
        mplsEroIPv4PrefixPrid        InstanceId, 
        mplsEroIPv4PrefixLen         Unsigned32, 
        mplsEroIPv4PrefixIPv4Addr    InetAddressIPv4 } 
 
mplsEroIPv4PrefixPrid OBJECT-TYPE 
    SYNTAX         InstanceId 
    STATUS         current 
    DESCRIPTION 
        "An integer index that uniquely identifies an instance of 
        the mplsEroIPv4PrefixEntry class." 
 
    ::= { mplsEroIPv4PrefixEntry 1 } 
 
mplsEroIPv4PrefixLen OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Length of Prefix in IPv4 Prefix ERO Subobject." 
 
    ::= { mplsEroIPv4PrefixEntry 2 } 
 
mplsEroIPv4PrefixIPv4Addr OBJECT-TYPE 
    SYNTAX         InetAddress 
    STATUS         current 
    DESCRIPTION 
        "IPv4 Prefix in IPv4 Prefix ERO Subobject." 
 
    ::= { mplsEroIPv4PrefixEntry 3 } 
 
 
-- 
-- IPv6 Address Prefix Subobject Table 
-- 
 
mplsEroIPv6PrefixTable OBJECT-TYPE 
    SYNTAX         SEQUENCE OF MplsEroIPv6PrefixEntry 
    PIB-ACCESS     install 
    STATUS         current 

    DESCRIPTION 
        "This table consists of MPLS IPv6 Prefix ERO Subobject 
        Entrees." 
 
    ::= { mplsEroClasses  2 } 
 
mplsEroIPv6PrefixEntry OBJECT-TYPE 
    SYNTAX         MplsEroIPv6PrefixEntry 
    STATUS         current 
    DESCRIPTION 
        "An instance of this class describes IPv6 Prefix ERO 
        Subobject. " 
 
    PIB-INDEX { mplsEroIPv6PrefixPrid } 
 
    ::= { mplsEroIPv6PrefixTable 1 } 
 
MplsEroIPv6PrefixEntry ::= SEQUENCE { 
        mplsEroIPv6PrefixPrid        InstanceId, 
        mplsEroIPv6PrefixLen         Unsigned32, 
        mplsEroIPv6PrefixIPv6Addr    InetAddressIPv6 } 
 
mplsEroIPv6PrefixPrid OBJECT-TYPE 
    SYNTAX         InstanceId 
    STATUS         current 
    DESCRIPTION 
        "An integer index that uniquely identifies an instance of 
        the mplsEroIPv6PrefixEntry class." 
 
    ::= { mplsEroIPv6PrefixEntry 1 } 
 
mplsEroIPv6PrefixLen OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Length of Prefix in IPv6 Prefix ERO Subobject." 
 
    ::= { mplsEroIPv6PrefixEntry 2 } 
 
mplsEroIPv6PrefixIPv6Addr OBJECT-TYPE 
    SYNTAX         InetAddress 
    STATUS         current 
    DESCRIPTION 
        "IPv6 Prefix in IPv6 Prefix ERO Subobject." 
 
    ::= { mplsEroIPv6PrefixEntry 3 } 
 
 
-- 
-- Autonomous System Number Subobject Table 
-- 
 
mplsEroASNumberTable OBJECT-TYPE 

    SYNTAX         SEQUENCE OF MplsEroASNumberEntry 
    PIB-ACCESS     install 
    STATUS         current 
    DESCRIPTION 
        "This table consists of MPLS Autonomous System Number ERO 
        Subobject Entrees." 
 
    ::= { mplsEroClasses  3 } 
 
mplsEroASNumberEntry OBJECT-TYPE 
    SYNTAX         MplsEroASNumberEntry 
    STATUS         current 
    DESCRIPTION 
        "An instance of this class describes Autonomous System 
        Number ERO Subobject. "                          
 
    PIB-INDEX { mplsEroASNumberPrid } 
 
    ::= { mplsEroASNumberTable 1 } 
 
MplsEroASNumberEntry ::= SEQUENCE { 
        mplsEroASNumberPrid        InstanceId, 
        mplsEroASNumberASNumber    Unsigned32} 
 
mplsEroASNumberPrid OBJECT-TYPE 
    SYNTAX         InstanceId 
    STATUS         current 
    DESCRIPTION 
        "An integer index that uniquely identifies an instance of 
        the mplsEroASNumberEntry class." 
 
    ::= { mplsEroASNumberEntry 1 } 
 
mplsEroASNumberASNumber OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Autonomous System Number in Autonomous System Number 
        Subobject." 
 
    ::= { mplsEroASNumberEntry 2 } 
 
-- 
-- ERO Table 
-- 
 
mplsEroTable OBJECT-TYPE 
    SYNTAX         SEQUENCE OF MplsEroEntry 
    PIB-ACCESS     install 
    STATUS         current 
    DESCRIPTION 
        "This table consists of MPLS ERO Subobject Entrees." 
 

    ::= { mplsEroClasses  4 } 
 
mplsEroEntry OBJECT-TYPE 
    SYNTAX         MplsEroEntry 
    STATUS         current 
    DESCRIPTION 
        "An instance of this class describes ERO Subobject." 
 
    PIB-INDEX { mplsEroPrid } 
 
    ::= { mplsEroTable 1 } 
 
MplsEroEntry ::= SEQUENCE { 
        mplsEroPrid        InstanceId, 
        mplsEroLoose       Unsigned32, 
        mplsEroSubObject   Prid } 
 
mplsEroPrid OBJECT-TYPE 
    SYNTAX         InstanceId 
    STATUS         current 
    DESCRIPTION 
        "An integer index that uniquely identifies an instance of 
        the mplsEroEntry class." 
 
    ::= { mplsEroEntry 1 } 
 
mplsEroLoose OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Loose Bit in ERO Subobject." 
 
    ::= { mplsEroEntry 2 } 
 
mplsEroSubObject OBJECT-TYPE 
    SYNTAX         Prid 
    STATUS         current 
    DESCRIPTION 
        "This points to an instance of one type of ERO subobject. It 
        could be an instance of mplsEroIpv4PrefixEntry,  
        mplsEroIpv6PrefixEntry or mplsEroASNumberEntry." 
 
    ::= { mplsEroEntry 3 } 
 
 
-- 
-- Ero Group Table 
-- 
 
mplsEroGroupTable OBJECT-TYPE 
    SYNTAX         SEQUENCE OF MplsEroGroupEntry 
    PIB-ACCESS     install 
    STATUS         current 

    DESCRIPTION 
        "This table defines ERO Subobject groups. Each group then is 
        used in an LSP definition. Grouping is done using a TagId  
        and order of Subobject in a group is provided by using a  
        precedence number." 
 
    ::= { mplsEroClasses  5 } 
 
mplsEroGroupEntry OBJECT-TYPE 
    SYNTAX         MplsEroGroupEntry 
    STATUS         current 
    DESCRIPTION 
        "An instance of ERO Subobject group." 
 
    PIB-INDEX { mplsEroGroupPrid } 
 
    ::= { mplsEroGroupTable 1 } 
 
MplsEroGroupEntry ::= SEQUENCE { 
        mplsEroGroupPrid           InstanceId, 
        mplsEroGroupId             TagId, 
        mplsEroGroupIdPrecedence   Unsigned32, 
        mplsEroGroupEroId          ReferenceId } 
 
mplsEroGroupPrid OBJECT-TYPE 
    SYNTAX         InstanceId 
    STATUS         current 
    DESCRIPTION 
        "An integer index that uniquely identifies an instance of 
        the mplsEroGroupEntry class." 
 
    ::= { mplsEroGroupEntry 1 } 
 
mplsEroGroupId OBJECT-TYPE 
    SYNTAX         TagId 
    STATUS         current 
    DESCRIPTION 
        "Tag Id (number) used to group multiple entries in this 
        table." 
 
    ::= { mplsEroGroupEntry 2 } 
 
mplsEroGroupIdPrecedence OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "This is used to provide ordering for entries with the same 
        Tag Id." 
 
    ::= { mplsEroGroupEntry 3 } 
 
mplsEroGroupEroId OBJECT-TYPE 
    SYNTAX         ReferenceId 

    PIB-REFERENCES { mplsEroEntry }  
    STATUS         current 
    DESCRIPTION 
        "Pointer to an instance of ERO Subobject. The ERO Subobject 
        with the same Id must be present." 
 
    ::= { mplsEroGroupEntry 4 } 
 
 
-- 
-- Preemption Classes 
-- 
 
mplsPreemptionClasses  OBJECT IDENTIFIER ::= { mplsSetupPib 5 } 
 
-- 
-- Preemption Table 
-- 
 
mplsPreemptionTable OBJECT-TYPE 
    SYNTAX         SEQUENCE OF MplsPreemptionEntry 
    PIB-ACCESS     install 
    STATUS         current 
    DESCRIPTION 
        "This table consists of LSP Preemption Entrees." 
 
    ::= { mplsFlowSpecClasses  1 } 
 
mplsPreemptionEntry OBJECT-TYPE 
    SYNTAX         MplsPreemptionEntry 
    STATUS         current 
    DESCRIPTION 
        "An instance of this class describes a LSP Preemption 
        object. " 
 
    PIB-INDEX { mplsPreemptionPrid } 
 
    ::= { mplsPreemptionTable 1 } 
 
MplsPreemptionEntry ::= SEQUENCE { 
        mplsPreemptionPrid       InstanceId, 
        mplsPreemptionSetupPrio  Unsigned32, 
        mplsPreemptionHoldPrio   Unsigned32 } 
 
mplsPreemptionPrid OBJECT-TYPE 
    SYNTAX         InstanceId 
    STATUS         current 
    DESCRIPTION 
        "An integer index that uniquely identifies an instance of 
        the mplsPreemptionEntry class." 
 
    ::= { mplsPreemptionEntry 1 } 
 

mplsPreemptionSetupPrio OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Indicates MPLS LSP Setup Priority." 
 
    ::= { mplsPreemptionEntry 2 } 
 
mplsPreemptionHoldPrio OBJECT-TYPE 
    SYNTAX         Unsigned32 
    STATUS         current 
    DESCRIPTION 
        "Indicates MPLS LSP Holding Priority." 
 
    ::= { mplsPreemptionEntry 3 } 
 
 
 
-- 
-- LSP Setup Classes 
-- 
 
mplsLspClasses  OBJECT IDENTIFIER ::= { mplsSetupPib 6 } 
 
 
-- 
-- LSP Table 
-- 
 
mplsLspTable OBJECT-TYPE 
    SYNTAX         SEQUENCE OF MplsLspEntry 
    PIB-ACCESS     install 
    STATUS         current 
    DESCRIPTION 
        "This table consists of MPLS LSP Entrees. Entries in this 
        table essentially point to instances of other PRCs such as  
        FEC, Label Request, ERO, Flow Spec and Preemption to form  
        complete LSPs." 
 
    ::= { mplsLspClasses  1 } 
 
mplsLspEntry OBJECT-TYPE 
    SYNTAX         MplsLspEntry 
    STATUS         current 
    DESCRIPTION 
        "An instance of MPLS LSP. " 
 
    PIB-INDEX { mplsLspPrid } 
 
    ::= { mplsLspTable 1 } 
 
MplsLspEntry ::= SEQUENCE { 
        mplsLspPrid        InstanceId, 

        mplsLspFec         Prid, 
        mplsLspLabReq      Prid, 
        mplsLspFlowSpec    Prid, 
        mplsLspPreemption  ReferenceId, 
        mplsLspEroList     TagReference } 
 
mplsLspPrid OBJECT-TYPE 
    SYNTAX         InstanceId 
    STATUS         current 
    DESCRIPTION 
        "An integer index that uniquely identifies an instance of 
        the mplsLspEntry class." 
 
    ::= { mplsLspEntry 1 } 
 
mplsLspFec OBJECT-TYPE 
    SYNTAX         Prid 
    STATUS         current 
    DESCRIPTION 
        "This points to an instance of one type of FEC. It could be 
        an instance of mplsFecIPv4HostAddrEntry,  
        mplsFecIPv6HostAddrEntry, mplsFecIPv4PrefixEntry,  
        mplsFecIPv6PrefixEntry, mplsFecASEntry." 
 
    ::= { mplsLspEntry 2 } 
 
mplsLspLabReq OBJECT-TYPE 
    SYNTAX         Prid 
    STATUS         current 
    DESCRIPTION 
        "This points to an instance of one type of Label Request  
        Object. It could be an instance of mplsLabReqGenericEntry, 
        mplsLabReqATMEntry, mplsLabReqFREntry." 
 
    ::= { mplsLspEntry 3 } 
 
mplsLspFlowSpec OBJECT-TYPE 
    SYNTAX         Prid 
    STATUS         current 
    DESCRIPTION 
        "This points to an instance of one type of FlowSpec. It  
        could be an instance of mplsFlowSpecCRLDPEntry, 
        mplsFlowSpecCLSEntry, mplsFlowSpecGSEntry." 
 
    ::= { mplsLspEntry 4 } 
 
mplsLspPreemption OBJECT-TYPE 
    SYNTAX         ReferenceId 
    PIB-REFERENCES { mplsPreemptionEntry }  
    STATUS         current 
    DESCRIPTION 
        "This points to an instance of mplsPreemptionEntry." 
 

    ::= { mplsLspEntry 5 } 
 
mplsLspEroList OBJECT-TYPE 
    SYNTAX         TagReference 
    PIB-TAG        { mplsEroGroupId }  
    STATUS         current 
    DESCRIPTION 
        "This references a Tag Id attribute in mplsEroGroup table.  
        All the entries in mplsEroGroup table that have this Tag Id  
        form the ERO List that is used for this LSP entry." 
 
    ::= { mplsLspEntry 6 } 
 
END    
