      SNMP-COMMUNITY-MIB DEFINITIONS ::= BEGIN

      IMPORTS
          IpAddress,
          MODULE-IDENTITY,
          OBJECT-TYPE,
          Integer32,
          snmpModules
              FROM SNMPv2-SMI
          RowStatus,
          StorageType
              FROM SNMPv2-TC
          SnmpAdminString,
          SnmpEngineID
              FROM SNMP-FRAMEWORK-MIB
          SnmpTagValue,
          snmpTargetAddrEntry
              FROM SNMP-TARGET-MIB
          MODULE-COMPLIANCE,
          OBJECT-GROUP
              FROM SNMPv2-CONF;

      snmpCommunityMIB MODULE-IDENTITY
          LAST-UPDATED "200308060000Z"        -- 06 Aug 2003, midnight
    ORGANIZATION "SNMPv3 Working Group"
    CONTACT-INFO "WG-email:   snmpv3@lists.tislabs.com
                  Subscribe:  majordomo@lists.tislabs.com
                              In msg body:  subscribe snmpv3

                  Co-Chair:   Russ Mundy
                              SPARTA, Inc
                  Postal:     7075 Samuel Morse Drive
                              Columbia, MD 21045
                              USA
                  EMail:      mundy@tislabs.com
                  Phone:      +1 410-872-1515

                  Co-Chair:   David Harrington
                              Enterasys Networks
                  Postal:     35 Industrial Way
                              P. O. Box 5005
                              Rochester, New Hampshire 03866-5005
                              USA
                  EMail:      dbh@enterasys.com
                  Phone:      +1 603-337-2614

                  Co-editor:  Rob Frye
                              Vibrant Solutions



                  Postal:     2711 Prosperity Ave
                              Fairfax, Virginia 22031
                              USA
                  E-mail:     rfrye@vibrant-1.com
                  Phone:      +1-703-270-2000

                  Co-editor:  David B. Levi
                              Nortel Networks
                  Postal:     3505 Kesterwood Drive
                              Knoxville, Tennessee 37918
                  E-mail:     dlevi@nortelnetworks.com
                  Phone:      +1 865 686 0432

                  Co-editor:  Shawn A. Routhier
                              Wind River Systems, Inc.
                  Postal:     500 Wind River Way
                              Alameda, CA 94501
                  E-mail:     sar@epilogue.com
                  Phone:      +1 510 749 2095

                  Co-editor:  Bert Wijnen
                              Lucent Technologies
                  Postal:     Schagen 33
                              3461 GL Linschoten
                              Netherlands
                  Email:      bwijnen@lucent.com
                  Phone:      +31-348-407-775
                 "

        DESCRIPTION
            "This MIB module defines objects to help support
             coexistence between SNMPv1, SNMPv2c, and SNMPv3.

             Copyright (C) The Internet Society (2003) This
             version of this MIB module is part of RFC 3584;
             see the RFC itself for full legal notices."

        REVISION "200308060000Z" -- 06 Aug 2003
        DESCRIPTION
            "Updated the LAST-UPDATED, CONTACT-INFO, and REVISION
             clauses and added a copyright notice to the
             DESCRIPTION clause of the MIB module's
             MODULE-IDENTITY invocation.

             Updated the description of snmpCommunityTransportTag
             to make it consistent with the rest of the document.

             Updated the description of `snmpTargetAddrMMS' to



             clarify that a value of 0 means that the maximum
             message size is unknown.

             Changed the name of 'snmpCommunityGroup' to
             snmpCommunityTableGroup to avoid a name conflict
             with the SNMPv2-MIB.

             Updated DESCRIPTION of snmpCommunityName.

             Updated DESCRIPTION of snmpTrapCommunity.

             Added snmpCommunityMIBFullCompliance.

             This version published as RFC 3584."

        REVISION "200003060000Z" -- 6 Mar 2000
        DESCRIPTION "This version published as RFC 2576."

    ::= { snmpModules 18 }

-- Administrative assignments ************************************

snmpCommunityMIBObjects
        OBJECT IDENTIFIER ::= { snmpCommunityMIB 1 }

snmpCommunityMIBConformance
        OBJECT IDENTIFIER ::= { snmpCommunityMIB 2 }

--
-- The snmpCommunityTable contains a database of community
-- strings.  This table provides mappings between community
-- strings, and the parameters required for View-based Access
-- Control.
--

snmpCommunityTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF SnmpCommunityEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "The table of community strings configured in the SNMP
         engine's Local Configuration Datastore (LCD)."
    ::= { snmpCommunityMIBObjects 1 }

snmpCommunityEntry OBJECT-TYPE
    SYNTAX       SnmpCommunityEntry
    MAX-ACCESS   not-accessible
    STATUS       current



    DESCRIPTION
        "Information about a particular community string."
    INDEX       { IMPLIED snmpCommunityIndex }
    ::= { snmpCommunityTable 1 }

SnmpCommunityEntry ::= SEQUENCE {
    snmpCommunityIndex               SnmpAdminString,
    snmpCommunityName                OCTET STRING,
    snmpCommunitySecurityName        SnmpAdminString,
    snmpCommunityContextEngineID     SnmpEngineID,
    snmpCommunityContextName         SnmpAdminString,
    snmpCommunityTransportTag        SnmpTagValue,
    snmpCommunityStorageType         StorageType,
    snmpCommunityStatus              RowStatus
}

snmpCommunityIndex OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The unique index value of a row in this table."
    ::= { snmpCommunityEntry 1 }

snmpCommunityName OBJECT-TYPE
    SYNTAX       OCTET STRING
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The community string for which a row in this table
         represents a configuration.  There is no SIZE constraint
         specified for this object because RFC 1157 does not
         impose any explicit limitation on the length of community
         strings (their size is constrained indirectly by the
         SNMP message size)."
    ::= { snmpCommunityEntry 2 }

snmpCommunitySecurityName OBJECT-TYPE
    SYNTAX       SnmpAdminString (SIZE(1..32))
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "A human readable string representing the corresponding
         value of snmpCommunityName in a Security Model
         independent format."
    ::= { snmpCommunityEntry 3 }

snmpCommunityContextEngineID OBJECT-TYPE



    SYNTAX       SnmpEngineID
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The contextEngineID indicating the location of the
         context in which management information is accessed
         when using the community string specified by the
         corresponding instance of snmpCommunityName.

         The default value is the snmpEngineID of the entity in
         which this object is instantiated."
    ::= { snmpCommunityEntry 4 }

snmpCommunityContextName OBJECT-TYPE
    SYNTAX       SnmpAdminString (SIZE(0..32))
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The context in which management information is accessed
         when using the community string specified by the
         corresponding instance of snmpCommunityName."
    DEFVAL      { ''H }   -- the empty string
    ::= { snmpCommunityEntry 5 }

snmpCommunityTransportTag OBJECT-TYPE
    SYNTAX       SnmpTagValue
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "This object specifies a set of transport endpoints
         which are used in two ways:
            - to specify the transport endpoints from which an
              SNMP entity will accept management requests, and
            - to specify the transport endpoints to which a
              notification may be sent using the community
              string matching the corresponding instance of
              snmpCommunityName.
         In either case, if the value of this object has
         zero-length, transport endpoints are not checked when
         either authenticating messages containing this community
         string, nor when generating notifications.

         The transports identified by this object are specified
         in the snmpTargetAddrTable.  Entries in that table
         whose snmpTargetAddrTagList contains this tag value
         are identified.

         If a management request containing a community string



         that matches the corresponding instance of
         snmpCommunityName is received on a transport endpoint
         other than the transport endpoints identified by this
         object the request is deemed unauthentic.

         When a notification is to be sent using an entry in
         this table, if the destination transport endpoint of
         the notification does not match one of the transport
         endpoints selected by this object, the notification
         is not sent."
    DEFVAL      { ''H }   -- the empty string
    ::= { snmpCommunityEntry 6 }

snmpCommunityStorageType OBJECT-TYPE
    SYNTAX       StorageType
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The storage type for this conceptual row in the
         snmpCommunityTable.  Conceptual rows having the value
         'permanent' need not allow write-access to any
         columnar object in the row."
    ::= { snmpCommunityEntry 7 }

snmpCommunityStatus OBJECT-TYPE
    SYNTAX       RowStatus
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The status of this conceptual row in the
         snmpCommunityTable.

         An entry in this table is not qualified for activation
         until instances of all corresponding columns have been
         initialized, either through default values, or through
         Set operations.  The snmpCommunityName and
         snmpCommunitySecurityName objects must be explicitly set.

         There is no restriction on setting columns in this table
         when the value of snmpCommunityStatus is active(1)."
    ::= { snmpCommunityEntry 8 }

--
-- The snmpTargetAddrExtTable
--

snmpTargetAddrExtTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF SnmpTargetAddrExtEntry



    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "The table of mask and maximum message size (mms) values
         associated with the snmpTargetAddrTable.

         The snmpTargetAddrExtTable augments the
         snmpTargetAddrTable with a transport address mask value
         and a maximum message size value.  The transport address
         mask allows entries in the snmpTargetAddrTable to define
         a set of addresses instead of just a single address.
         The maximum message size value allows the maximum
         message size of another SNMP entity to be configured for
         use in SNMPv1 (and SNMPv2c) transactions, where the
         message format does not specify a maximum message size."
    ::= { snmpCommunityMIBObjects 2 }

snmpTargetAddrExtEntry OBJECT-TYPE
    SYNTAX       SnmpTargetAddrExtEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Information about a particular mask and mms value."
    AUGMENTS       { snmpTargetAddrEntry }
    ::= { snmpTargetAddrExtTable 1 }

SnmpTargetAddrExtEntry ::= SEQUENCE {
    snmpTargetAddrTMask              OCTET STRING,
    snmpTargetAddrMMS                Integer32
}

snmpTargetAddrTMask OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..255))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The mask value associated with an entry in the
         snmpTargetAddrTable.  The value of this object must
         have the same length as the corresponding instance of
         snmpTargetAddrTAddress, or must have length 0.  An
         attempt to set it to any other value will result in
         an inconsistentValue error.

         The value of this object allows an entry in the
         snmpTargetAddrTable to specify multiple addresses.
         The mask value is used to select which bits of
         a transport address must match bits of the corresponding
         instance of snmpTargetAddrTAddress, in order for the



         transport address to match a particular entry in the
         snmpTargetAddrTable.  Bits which are 1 in the mask
         value indicate bits in the transport address which
         must match bits in the snmpTargetAddrTAddress value.
         Bits which are 0 in the mask indicate bits in the
         transport address which need not match.  If the
         length of the mask is 0, the mask should be treated
         as if all its bits were 1 and its length were equal
         to the length of the corresponding value of
         snmpTargetAddrTable.

         This object may not be modified while the value of the
         corresponding instance of snmpTargetAddrRowStatus is
         active(1).  An attempt to set this object in this case
         will result in an inconsistentValue error."
    DEFVAL { ''H }
    ::= { snmpTargetAddrExtEntry 1 }

snmpTargetAddrMMS OBJECT-TYPE
    SYNTAX      Integer32 (0|484..2147483647)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The maximum message size value associated with an entry
         in the snmpTargetAddrTable.  Note that a value of 0 means
         that the maximum message size is unknown."
    DEFVAL { 484 }
    ::= { snmpTargetAddrExtEntry 2 }

--
-- The snmpTrapAddress and snmpTrapCommunity objects are included
-- in notifications that are forwarded by a proxy, which were
-- originally received as SNMPv1 Trap messages.
--

snmpTrapAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of the agent-addr field of a Trap PDU which
         is forwarded by a proxy forwarder application using
         an SNMP version other than SNMPv1.  The value of this
         object SHOULD contain the value of the agent-addr field
         from the original Trap PDU as generated by an SNMPv1
         agent."
    ::= { snmpCommunityMIBObjects 3 }




snmpTrapCommunity OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of the community string field of an SNMPv1
         message containing a Trap PDU which is forwarded by a
         a proxy forwarder application using an SNMP version
         other than SNMPv1.  The value of this object SHOULD
         contain the value of the community string field from
         the original SNMPv1 message containing a Trap PDU as
         generated by an SNMPv1 agent.  There is no SIZE
         constraint specified for this object because RFC 1157
         does not impose any explicit limitation on the length
         of community strings (their size is constrained
         indirectly by the SNMP message size)."
    ::= { snmpCommunityMIBObjects 4 }

-- Conformance Information **************************************

snmpCommunityMIBCompliances OBJECT IDENTIFIER
                            ::= { snmpCommunityMIBConformance 1 }
snmpCommunityMIBGroups      OBJECT IDENTIFIER
                            ::= { snmpCommunityMIBConformance 2 }

-- Compliance statements

snmpCommunityMIBCompliance MODULE-COMPLIANCE
    STATUS       current
    DESCRIPTION
        "The compliance statement for SNMP engines which
         implement the SNMP-COMMUNITY-MIB."

    MODULE       -- this module
        MANDATORY-GROUPS { snmpCommunityTableGroup }

        OBJECT           snmpCommunityName
        MIN-ACCESS       read-only
        DESCRIPTION     "Write access is not required."

        OBJECT           snmpCommunitySecurityName
        MIN-ACCESS       read-only
        DESCRIPTION     "Write access is not required."

        OBJECT           snmpCommunityContextEngineID
        MIN-ACCESS       read-only
        DESCRIPTION     "Write access is not required."




        OBJECT           snmpCommunityContextName
        MIN-ACCESS       read-only
        DESCRIPTION     "Write access is not required."

        OBJECT           snmpCommunityTransportTag
        MIN-ACCESS       read-only
        DESCRIPTION     "Write access is not required."

        OBJECT           snmpCommunityStorageType
        MIN-ACCESS       read-only
        DESCRIPTION     "Write access is not required."

        OBJECT           snmpCommunityStatus
        MIN-ACCESS       read-only
        DESCRIPTION     "Write access is not required."

    ::= { snmpCommunityMIBCompliances 1 }

snmpProxyTrapForwardCompliance MODULE-COMPLIANCE
    STATUS       current
    DESCRIPTION
        "The compliance statement for SNMP engines which
         contain a proxy forwarding application which is
         capable of forwarding SNMPv1 traps using SNMPv2c
         or SNMPv3."
    MODULE       -- this module
        MANDATORY-GROUPS { snmpProxyTrapForwardGroup }
    ::= { snmpCommunityMIBCompliances 2 }

snmpCommunityMIBFullCompliance MODULE-COMPLIANCE
    STATUS       current
    DESCRIPTION
        "The compliance statement for SNMP engines which
         implement the SNMP-COMMUNITY-MIB with full read-create
         access."

    MODULE       -- this module
        MANDATORY-GROUPS { snmpCommunityTableGroup }
    ::= { snmpCommunityMIBCompliances 3 }

snmpCommunityTableGroup OBJECT-GROUP
    OBJECTS {
        snmpCommunityName,
        snmpCommunitySecurityName,
        snmpCommunityContextEngineID,
        snmpCommunityContextName,
        snmpCommunityTransportTag,
        snmpCommunityStorageType,



        snmpCommunityStatus,
        snmpTargetAddrTMask,
        snmpTargetAddrMMS
    }
    STATUS       current
    DESCRIPTION
        "A collection of objects providing for configuration
         of community strings for SNMPv1 (and SNMPv2c) usage."
    ::= { snmpCommunityMIBGroups 1 }

snmpProxyTrapForwardGroup OBJECT-GROUP
    OBJECTS {
        snmpTrapAddress,
        snmpTrapCommunity
    }
    STATUS       current
    DESCRIPTION
        "Objects which are used by proxy forwarding applications
         when translating traps between SNMP versions.  These are
         used to preserve SNMPv1-specific information when
         translating to SNMPv2c or SNMPv3."
    ::= { snmpCommunityMIBGroups 3 }

END
