# -*- text -*-
##############################################################################
#
#  Riverstone Networks' RADIUS VSAs
#  *** For RapidOS Versions 9.1 and above ONLY ***
#
#  $Id: dictionary.riverstone 28946 2009-07-06 12:39:58Z wmeier $
#
##############################################################################

VENDOR		Riverstone			5567

#
#  Riverstone-Command
#
#  This attribute is sent in Accounting-Requests, and contains text
#  from the admin's CLI session.
#
BEGIN-VENDOR	Riverstone

ATTRIBUTE	Riverstone-Command			1	string

#
#  This attribute is sent in Accounting-Requests, as a duplicate
#  of syslog for system event messages.
#
ATTRIBUTE	Riverstone-System-Event			2	string

#
#  This attribute is sent in Accounting-Requests, to log changes
#  made via SNMP.
#
ATTRIBUTE	Riverstone-SNMP-Config-Change		3	string

#
#  This attribute should be sent in Access-Accept packets, to set
#  the privilege level.  It MUST be sent when the device is operating
#  in Mult-User Access mode.
#
ATTRIBUTE	Riverstone-User-Level			4	integer

END-VENDOR	Riverstone
